|  |  |  |
| --- | --- | --- |
| Bochs User Manual | | |
| [Prev](http://docs.google.com/bios-tips.html) | Chapter 8. Tips and Techniques | [Next](http://docs.google.com/vesa-notes.html) |

8.17. How to enter special key combination

Your window manager may trap the key combination you want to enter in Bochs guest OS, for example **control**+**alt**+**delete**. Here is a work-around:

Press and hold **control**+**alt**, move your mouse cursor outside of the Bochs window. Release them, move the cursor back in the Bochs window and press **delete**.

This should work for any key combination.

If you need one key combination frequently, set it up as user key combination with the [keyboard](http://docs.google.com/bochsrc.html#BOCHSOPT-KEYBOARD) option in your configuration file. This key combination is sent to the guest OS when you press the user button in the [headerbar](http://docs.google.com/textconfig.html#HEADERBAR). Depending on the used [display\_library option](http://docs.google.com/bochsrc.html#BOCHSOPT-DISPLAYLIBRARY), it may even be possible to edit the shortcut before sending it.

|  |  |  |
| --- | --- | --- |
| [Prev](http://docs.google.com/bios-tips.html) | [Home](http://docs.google.com/index.html) | [Next](http://docs.google.com/vesa-notes.html) |
| BIOS Tips | [Up](http://docs.google.com/howto.html) | Notes about VESA usage |